****

**Project 2.14**

**Electric Power Consume Management**

Student ID: GT60708

Full name: Nguyen Tien Khoa

**Introduction**

Vietnamese Electric Power Company has some problem to collect data from consume monitor device. So, they need a program to collect data information from those device quicker and cheaper. The program should support to get data about electric consume on monitor device though internet. Moreover, It can help customers to be aware about electric bill. Therefore, company can track consume electric of their customer then give good advices.

Because of using internet to collect data, the system must provide a sever. And all device must to have internet connection. But, device works 24/7 to monitor electric consuming, internet connection would be interrupted and device would be down sometimes by some reason. So, server should have a strategy to deal with offline device.

Surely, monitor devices are not perfect. They may be offline, conflict data, dirty data, etc. So, server should be save these problems to write report. Report will be read by administrators, the electric engineers. Then, they can track to solve problems faster and better. Therefore, the new system will satisfy customer and improve productivity and quality.

In short, the new system manage monitor device to collect data from customer then print it to report. It helps Vietnamese electric company manage and support electric consuming customers.

**Open point**

Customers regard to their money, product and service. Example, they need to know when electric bill become expensive, why electric lost, etc. So, system should have sms, email or something to notify customer about their information.

Customers should able to use the new system to interact and discuss about problems and needs.

**Analysis**

Base on requirement of this project and my experiences in Java, Java programming language is used to develop. Focus on available tools, low price and fast development, this project includes 3 modules to contain web service, device simulator and share project.

Web service, this is the main project.

Device simulator, this is project to simulate real device. Actually, I don't have any real device, this simulator would support to make system be visible.

Share project, this contain model classes, constant is used by both service and device.

**Resources analysis**

**Human resources:**

This project is a personal coursework, therefore I plan to develop by one Java developer.

**Time resources:**

Deadline is November 24, 2016

**Tools resources:**

This project focus on education, so I should be a freeware.

Java programming language is used to develop, because there are a lot free Java frameworks and libraries.

MySQL Database has community version is free to download.

A linux OS works faster with Java, and It is free.

**Requirement analysis**

Program must use java open source technique for keeping low price.

Program must delivery within 3 months with main functions.

Program must use an incremental development model for integrating other requirements.

Program must allow device to register into system automatically.

Program must be limited access, Administrator only on this version.

Program must allow admin to modify customer data.

Program must have a report reviewer, such as dashboard.

Program must have calculator to built electric bill on demand.

Program should validate device information to track problems on devices.

Program would allow admin to modify consume policy data.

Program would allow administrator edit some properties on device.

Program should allow to register new user account.

Program should update device on database when device reconnect.

Program should poll device every 10 minutes, in this version.

Device Simulator should able to simulate a device error.

Device Simulator should able to be polled by server.

Device Simulator should able to send data to server.

Device Simulator should able to store data in internal memory, such as files.

**Technology analysis**

**Srping Framework:** System must have server to provide service. With the main target is quicker and cheaper, using open source library to build the service. Spring framework seem to be the good choice with wide technique support and easy to use.

**Runable JAR:** In this article, monitor device is not developed and built so that a virtual device run on JVM is using to simulate real device. I considered to use Spring Shell, but It is a bit heavy with this requirement and I have no experience. So Spring Shell will be expensive.

**Java Message Service (JMS) and Active MQ:** Deep knowledge about Network is not require. For connection between device and server, JMS is good technique. ActiveMQ service is build to store, forward and broadcast to device and receive message from devices. Device and server just connect to ActiveMQ for communication through IP Address, port and protocol of ActiveMQ server broker.

**JavaScript Object Notation (JSON):** There is no important personal information is used. So, JSON is consider to used to convert Java Object to Text for transfer in communication. The reason are easy to use, easy to read, fast speed, light weight. Jackson JSON is used instead of Google GSON because of speed and feature powerful.

**Java Sevlet Facet (JSF) and Primeface:** It is famous of powerful and less javascript technology. For user interface, javascript is difficult to Java developer like me. Primeface framework is supported to integrate with Spring framework by Srping webflow library. So, with a bit javacript knowledge and time to research spring webflow and Primeface, JSF is considered to be best choice to build UI.

**MySQL:** System have Database server to store device information and customer information. MySQL is used to build a databse server. In future, with a huge database, the service should separate into 2 server, one other will use No-SQL data like mongoDB for lighter and faster query device information. Because the security and restrains on device information is not import.

**Hibernate:** It is a famous framework support Java Persistence Access(JPA). There is no reason to avoid Hibernate, this easy to use and powerful. But, I consider to remove it when separate data into SQL Database and No SQL database. In this case, Spring Database is good choice to support JPA because It supported both JPA and MongoDB

**Spring webflow and JSF:** As I mentioned in JSF, Spring webflow is the solution to integrate JSF with Spring web mvc. Spring web mvc and JSF are 2 difference framework use Model View Controller (MVC) Architecture, so that they need a midleware to work together. Moreover, Spring webflow also support to control life cycle and navigation such as define variable and view, follow step and check state. In this version, I just use Spring webflow to integrate Spring web mvc and jsf, especially Primeface.

**Spring Security:** Spring security support protect server from unexpected access. Encryption is support by Spring security by many algorithm such as MD5 on 32 characters and Bcrypt on 64 characters. Of course, It supports access with JPA database.

**Design**

**­­Use case Diagram**

User can access in to system through authentication system. After that, user with role "ADMIN" can change device information, change customer information, change policy setting, poll device and check consume bill.

Data storage is use to store information of devices, settings and customer.

System process request from users and devices. Then, the result is store in data storage.

System collects and calculates information of device for providing chart report to user.

**Workflow diagrams**

**Data flow:**



- Data is store in data server MySQL, EPCM System access and save data to data server.

- EPCM System sends message to Device through JMS broker. JMS broker is ActiveMQ server, store and forward message from system to device. Actually, System send a broadcast message to broker with mac Address of device contained in message header. Then, message is received by device has mac address same as mac Address in message header.

- Agent is software run on device. It helps device send and receive message.

- Monitor device use agent for send request to System. Message is receive by ActiveMQ server then forward to system. In case, device response a request, message is sent to a temporary destination create by requester.

For more information, please read Appendix A session JMS Topic and Queue.

**Authentication flow:**



Workflow of user authentication and authorization. Step to get access to management system.

User login to system by providing login information. System check login information from request, if invalid information, system show error message. When information is corrected, system checks role, if user has not role admin, system show access denied message. When use has admin permission, it go to management page. User can log out, to go to login page.

**Change device data flow:**



Workflow of Changing Device Information by system.

User change device on system and do save new device information. New device information will be saved into database. Then a message is send to device for requesting update new device info. In case device is offline, message is stayed on broker until device get connection and get the request message. For dirty prevent, ActiveMQ messages have "time to live" attribute to detect out of date message.

In case, User remove device from manager list, device just been removed from manager list. There is no request to device after device is remove from the list. When have request contains device info from device, device is registered into system again. Receive data flow diagram will discuss about process message from devices.

**Poll device data flow:**



Workflow fo poll device data. Poll device is request device report it status and send it data to EPCM System.

When user do poll devices on management list. Message is sent to broadcast and wait for response from receiver. Each message has time to live. After 10 second, if there is no device receives and responses, system save polled devices is down with status offline and ip address is release, e.g "0.0.0.0" . If message response in 10 second, system will show polling progress for this devices is success. Devices will send its information device after that. Receive data flow diagram will discuss about process message from devices.

**Receive device data flow:**



Workflow of process when system receive data from devices.

When message is receive on system, system will detect type of data.

In case, message is a device basic information, system tried to find confliction with old data such as, consume number is lower, device's ip address conflict with other one. If there is conflictions, System create notification for those devices have conflictions and save into database. After that device is save into database with as a new device or a old one base on mac address.

In case, message is a device notification, a new device notification is create and save into database.

Open point, Notification should check existed of device or device will send a basic info message before send device notification for ensure that notification is searchable by device.

**Class Diagrams**

**Implement**

**Maintenance**